Successive FRDM enhancements

Optimization (2006)

Better search for optimum FRDM parameters. Accuracy improvement: 0.01 MeV

New mass data base (AME2003) (2006) Better agreement than with AME1989. Accuracy improvement: 0.04 MeV

Full 4D energy minimization (2006–2008) Full 4D minimization(ϵ2, ϵ3, ϵ4, ϵ6) step=0.01. Accuracy improvement: 0.02 MeV

Axial asymmetry (2002–2006)

Also yields correct SHE gs assignments. Accuracy improvement: 0.01 MeV

L variation (2009–2011)

Accuracy improvement: 0.02 MeV

Improved gs correlation energies (2012) Accuracy improvement: 0.01 MeV